### Failsafe Settings

Instruction
Failsafe is one of the advanced functions for the autopilot system. If this fuction is selected, Failsafe will be triggered when the Main Controller loses the control signal. The multi-rotor will automatically land if the Failsafe mode is active, or return to home if in GPS mode using the GPS module.
Important
If you select the "Go-Home and Landing" function, please make sure to connect to the GPS module correctly and record the home point successfully, since the autopilot system has to know the home point when going home.