### Intelligent Orientation Control (IOC)

IOC Setting Procedure

1. Please choose a 3-positions switch on your transmitter as IOC switch, which is also used for recording the multi-rotor orientation or home position.
2. Make sure to connect the correct receiver channel to X2 port of MC.
3. Click the CheckBox to enable the IOC.
4. Select control mode options.
5. Toggle the IOC switch to move the cursor of X2 to turn the corresponding area blue respectively.

Tips

1. If you use S-Bus/PPM receiver, the default X2 channel connection is the 6th channel of the transmitter.
2. If the software does not give the correct response, use end-point fine tuning on your transmitter to adjust the X2 channel.
3. Refer to the Manual for operation info.