### R/C TX & RX Settings

R/C TX Setting

1. Please select the model type of the TX as AERO.
2. Set all curves (pitch, throttle, expo, rates, etc) as default. Set the endpoints of all channels to default values (100%) and all trims and sub-trims to zero.

TX Sticks Calibration

1. Click the START button and then move all of the TX sticks throughout their complete travel range several times.
2. Once the above procedure is complete, click the FINISH button.

Important
If you change the travel adjust of the TX, please redo the above Calibration.