### R/C TX & RX Settings

Control Mode Setting

1. Choose a 3-position switch channel for the mode selection.
2. While watching the U channel slider in the assistant software, at each switch position, use the TX sub-trim and end-point to move the U channel slider until the GPS, Atti. or Manual area turns blue.
3. Set the Failsafe of the TX.
4. Select a Mode from the Drop-down box. If "FailSafe" chosen, the system enters into FailSafe by toggling the switch.

After setup please re-check

1. Toggle the mode switch and make sure the relevant area of the U channel slider turns blue.
2. Switch off the TX, the Failsafe part of the U channel slider should turn blue.

Tip
Please refer to your TX manual and "F/S" in the "Advanced" for more setting details.