### Gimbal Setting

Manual Control Speed

Manual Control Speed determines the gimbal reaction from the transmitter.

Setting Procedure

1. You should assign one of the knobs on your transmitter to the X1 channel for controlling the Pitch direction (angle) of camera gimbal during flight.
2. Adjust the reaction speed of pitch. The bigger the value the quicker the gimbal reaction.

Important

1. If parameter adjustment was enabled on channel X1, the gimbal manual control via channel X1 will still be on as well. Do not use X1 to control gimbal pitch and remote adjust parameters at the same time.
2. Please reset the Gain parameters in the Basic section if there is flight jitter after gimbal is mounted.