### Gimbal Setting

If you use a gimbal, please configure the parameters on this page.
This system supports 2-axis gimbals with servo with a 1520us center point. Make sure the connection is correct.
Important
If you enable the gimbal control in assistant software during the configuration, please note that there will be outputs from F1 and F2 ports. NEVER connect F1/F2 to ESCs wired to motors with propellers.