### Flight Limits

Distance Limit

If distance restriction is needed, please click ON and write a value (Range: 30~500m) in the Max Radius box, so that the distance from the aircraft to the Home-point will not be longer than the max-radius you set. The Distance Restriction function ONLY works in GPS ATTI. Mode. The aircraft may fly out of the restriction when emergency brake is carried out at the border (the buffer zone is about 10m), if it flies out of the restricted distance the Control Mode LED will blink Cyan. However, the Failsafe and the Ground Station operation are not restricted to this distance limit. If no distance limit is needed, please click OFF.