### Failsafe Settings

Please select the desired Failsafe method.

What is Enhanced Failsafe
Using the GPS Module, you can select "Landing" or "Go-Home and Landing"(in GPS Mode). Otherwise, only Landing.It will be triggered when the Main Controller (MC) loses the control signal from the TX.

What is Home point
Before takeoff, current position of multi-rotor will be saved as home point when you push the throttle stick first time, after 6 or more GPS satellites are acquired, for more than 8s. Assure correct recording.

How to re-gain control
Switch to Manual Mode or Atti. Mode to re-gain control of multi-rotor when it is in Failsafe Mode.

Important
The aircraft will not go home if the GPS signal is not good.