### R/C TX & RX Settings

X1/X2 Channel Monitor

This step is optional. If it is necessary for you, please setup the channel on your R/C TX correctly, and then you can monitor the X1 and X2 Channels on this page.

Tips

1. X1 Channel is for remote gain tuning or gimbal pitch control(e.g. DJI H3-2D Gimbal).
2. Carry out X1 Calibration if X1 Channel is used for H3-2D gimbal pitch control.
3. X2 Channel is for remote gain tuning or Intelligent Orientation Control (IOC), or as S-Bus input.