You¡¯ve chose parameters tuning by X1/X2 channel with Tx Knob, but no signal detected on X1/X2 input channel,or Tx didn¡¯t powered on.<br />1.Power on the Tx.2.Connect the X1/X2 channel;3.Disable all knob tuning.