### Gimbal Setting

Servo Travel Limit

MAX/MIN are servo travel limits; adjust them to avoid mechanical binding.

Setting Procedure

1. Place your multi-rotor on level ground.
2. Adjust MAX/MIN value of PITCH and ROLL direction. Make sure to avoid mechanical binding when the gimbal is moving.
3. Adjust Center value of PITCH and ROLL direction to make the camera mounting frame to your desired angle-to-ground.

Important
If servo expansion is used, which may enlarge the servo travel limit, make sure to reset your servo travel limit.