1. Please make your selection according to your multi rotor type.We have following built-in types:
2. Make sure the rotation direction of each motor is the same as the way the figure shows in our assistant software.If not, switch any of two wire connections of the incorrect motor.
3. Make sure the type of propeller matches the rotation direction of motor.
4. You have to set your transmitter to ACROBATIC Mode.