### Gimbal Setting

Automatic Control Gain

Automatic Control Gain determines the gimbal reaction controlled by the autopilot system. The bigger the value the quicker the gimbal reaction. If the gain is too large, you will find the gimbal oscillating in the corresponding direction.

Adjust Procedure

Adjust the gain of the automatic control. The initial value of 100.00 is the maximum angle. The bigger the gain, the bigger the reaction angle. Click the REV /NORM button, to reverse the feedback control directions.