### Motor Settings

What is Motor Idle Speed
Motor Idle Speed is the lowest speed after motors start. There are five levels from LOW speed to HIGH speed, and the default is RECOMMENDED.

How to set
Click the corresponding level to select Motor Idle Speed. RECOMMENDED is the advised level. Set to LOW, the motor idle speed will be lowest.Set to HIGH, the motor idle speed will be highest. You can set it according to the individual requirement.

Important
For users whose aircraft takes off at a lower throttle position, please set the idle speed at a low level. For common users, set it to RECOMMENDED or above, since setting idle speed too low may affect motor(s) spool up.