### Motor Settings

Push both sticks to the left bottom or right bottom to start the motors. A different Cut Off Type stops the motor in a different way. Refer to the NAZA-M Quick Start Guide for more details.

Immediately In any control mode, once motors start and throttle stick is over 10%, motors will stop immediately when throttle stick is back under 10% again.In this case, if you push the throttle stick over 10% within 5 seconds after motors stop, motors will re-start. If you don’t push throttle stick after motors start in 3 seconds, motors will stop automatically.

Intelligent In any control mode, only push both sticks to the left or right bottom can stop motors.In ATTI./GPS Mode, any one of following cases will stop motors. (1)You don’t push throttle stick after motors start within 3 seconds. (2)Throttle stick under 10%, and after landing 3 seconds. (3)The slope angle of multi-rotor is over 70°, and throttle stick under 10%.